Approved by \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 **Town of Apple Valley**

 **Division of Building and Safety/Engineering**

 **GRADING INSPECTION REPORT**

OWNER: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ PERMIT NO.: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

ADDRESS OR TRACT NO.: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

[ ]  **ROUGH GRADING INSPECTION:**

[ ]  **By Soils Engineer**

Over-excavation and fills were installed upon properly prepared base material and compacted in

compliance with Section 1804C.B.C. and where the report of an engineering geologist has recommended.

Lot Nos.: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

See attached report for compaction test data, recommended allowable soil bearing values and other

special recommendations.

EXPANSIVE SOILS [ ]  YES [ ]  NO Lot Nos.: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Engineer Name (print): \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Engineer (signature): \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Reg. No.: \_\_\_\_\_\_\_\_ Phone No.: \_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_

[ ]  **By Grading Contractor**

The rough grading has been completed in accordance with the approved plans including: drainage devices;

grading to approximate final elevations; swales and terraces ready for paving; berms installed; required

drainage slopes provided; and where reports of an engineering geologist and/or soils engineer have been

prepared, the recommendations contained therein have been followed.

Lot Nos.: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Remarks: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Contractor Name (print): \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Contractor (signature): \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Lic. No.: \_\_\_\_\_\_\_\_ Phone No.: \_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_

[ ]  **FINAL GRADING INSPECTION:**

The grading has been satisfactorily completed in accordance with the approved plans. All required

drainage devices have been installed; slope planting established and adequate provisions have been made

for drainage of surface waters from each building site. The recommendations of the soils engineer and/or

engineering geologist (if such persons were employed) have been incorporated in the work.

Lot Nos.: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Engineer Name (print): \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Engineer (signature): \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Reg. No.: \_\_\_\_\_\_\_\_ Phone No.: \_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_